GARAGE SECTIONAL

7” MINIMUM

EMBEDMENT

4X8X16 BLOCK

TYPICAL

ROOF COVERING

TYPE

THICKNESS “

FOOTING TYPE

WIDTH (MIN 12”)

DEPTH (MIN 42”)

FLOOR TYPE

SHEATHING TYPE

SIZE

STUD SIZE 2 X ”

STUD SPACING ” O.C.

 SIZE

SILL PLATE ATTACHMENT

TYPE SIZE

SPACING

TREATED SILL PLATE SIZE

2 X ”

 SIDING TYPE

WALL HEIGHT FT.

TRUSS TO WALL CONNECTOR TYPE

TRUSS SPACING O.C.

SHEATHING TYPE

SIZE

UNDERLAYMENT

TYPE

GARAGE LAY OUT

ENTRY DOOR SIZE

 X

DEPTH FT

WIDTH FT

TRUSS DIRECTION

WIDTH

DEPTH

SHOW ALL DOORS AND WINDOW LOCATIONS

WINDOW SIZE

 X

HEADER SIZE

 X

OVERHEAD DOOR SIZE

 X

DEPTH

WIDTH

